Standard Setup:

* Input lines are labelled green.
* Run from the Arduino to the input section on the bread board.